1. **Species and its %:**

1. Hardwood species, Moisture content about 50%, AD, Green

|  |  |
| --- | --- |
| Sapelli | 1000~2000 m3/m |
| Kosipo | 50 m3/m |
| Sipo | 25 m3/m |
| Padouk | 25 m3/m |
| Iroko  | 10 m3/m |

**2. Specification of the boards:**

|  |  |
| --- | --- |
| Thickness, mm | Preferred from 58 to 100 |
| Width, mm | 100-149 – 10%, 150 and wider 90%. |
| Length, m | From 2.2 to 5.0 with the interval from 200 mm or 300 mm, Such as 2.2/2.4/2.6/2.8/3.0/3.3/3.6/3.8/4.0/4.2/4.4/4.7/5.0 |

**3. Specification of the short cant:**

|  |  |
| --- | --- |
| Length, m | 0.9/1.8 and as agreed |
| Size, mm | 50x50 ~ 90x90 and as agreed, it requires the negotiations. |

**4. Specification of the long cant:**

|  |  |
| --- | --- |
| Length, m | 2.2 / 2.5 / 2.6 – inquiries are welcome. |
| Size, mm | 100х100 |

The size of the cant depends on the size of the boards ordered for production.

The allowance for the thickness is 5 mm and for the length is 50 mm.

The allowance for the width is to be fixed by the Parties.

Total per month: up to 2 100 m3

1. **Terms of Trading**

Loading ports : Sea port of Douala and/or Kribi, Cameroon, depending on the Buyer’s request.

Terms of Delivery : FOB and/or FCA Incoterms 2020

Minimum quantity : 1 (one) container in case of a trial order, the quantity per container is about 25 m3.

Terms of Payment and other Terms are to be discussed, we are quite flexible to enter the negotiations.